,Product Model Number##OTHER##,ProductCode##OTHER##,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Efficiency Rating##OTHER##,Head##PIPING_PRESSURE##FEET_OF_WATER,Flow##PIPING_FLOW##CUBIC_METERS_PER_HOUR,Suction Connection diameter##LENGTH##MILLIMETERS,Discharge Connection diameter##LENGTH##MILLIMETERS,Material##OTHER##,Wattage##ELECTRICAL_APPARENT_POWER##KILOWATTS,Connection Type##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Full Load Amperes##ELECTRICAL_CURRENT##AMPERES,Product Range##OTHER##,z OR##LENGTH##MILLIMETERS,z OL##LENGTH##MILLIMETERS,z BR##LENGTH##MILLIMETERS,z BL##LENGTH##MILLIMETERS,z BH##LENGTH##MILLIMETERS,z LL##LENGTH##MILLIMETERS,z IR##LENGTH##MILLIMETERS,z IL##LENGTH##MILLIMETERS,z IH##LENGTH##MILLIMETERS,z SN##LENGTH##MILLIMETERS,z DN##LENGTH##MILLIMETERS,z SF##LENGTH##MILLIMETERS,z DF##LENGTH##MILLIMETERS,z ML##LENGTH##MILLIMETERS
MAGNA3 D 65-150 F_60_98126863,98126863,MAGNA3 D 65-150 F,60,0.17,49.21,42.5,65,65,CAST IRON,1301,GF,208,5.68,UUPEFAM,130.00,130.00,228.00,228.00,77.00,340.00,0,130.00,0,65.00,65.00,65.00,65.00,312.00
MAGNA3 D 80-100 F_60_98126864,98126864,MAGNA3 D 80-100 F,60,0.17,32.81,61,80,80,CAST IRON,1052,GF,208,4.62,UUPEFAM,130.00,130.00,244.00,244.00,97.00,360.00,164.00,130.00,115.00,80.00,80.00,80.00,80.00,318.00
MAGNA3 D 100-120 F_60_98126865,98126865,MAGNA3 D 100-120 F,60,0.17,39.37,71,100,100,CAST IRON,1582,GF,208,6.98,UUPEFAM,135.00,135.00,252.00,252.00,103.00,450.00,0,135.00,0,100.00,100.00,100.00,100.00,330.00
